# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal lines have 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
#  for emulated keyboards that have only one shift key, set both LSHIFT
#  and RSHIFT to the same row/col and use RSHIFT for VSHIFT and SHIFTL.
# '!LCTRL row col'       left control keyboard row/column
# '!VCTRL ctrlkey'       virtual control key (LCTRL)
# '!LCBM row col'        left CBM keyboard row/column
# '!VCBM cbmkey'         virtual CBM key (LCBM)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have these values, flags can be ORed to combine them:
# 0x0000      0  key is not shifted for this keysym/scancode
# 0x0001      1  key is combined with shift for this keysym/scancode
# 0x0002      2  key is left shift on emulated machine
# 0x0004      4  key is right shift on emulated machine (use only this one
#                for emulated keyboards that have only one shift key)
# 0x0008      8  key can be shifted or not with this keysym/scancode
# 0x0010     16  deshift key for this keysym/scancode
# 0x0020     32  another definition for this keysym/scancode follows
# 0x0040     64  key is shift-lock on emulated machine
# 0x0080    128  shift modifier required on host
# 0x0100    256  key is used for an alternative keyboard mapping, e.g. C64 mode in x128
# 0x0200    512  alt-r (alt-gr) modifier required on host
# 0x0400   1024  ctrl modifier required on host
# 0x0800   2048  key is combined with cbm for this keysym/scancode
# 0x1000   4096  key is combined with ctrl for this keysym/scancode
# 0x2000   8192  key is (left) cbm on emulated machine
# 0x4000  16384  key is (left) ctrl on emulated machine
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key (x128)
# 'keysym -4 1' CAPS (ASCII/DIN) key (x128)
# 'keysym -5 n' joyport keypad, key n (not supported in x128)
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Positional Mapping, TR Layout, C64, GTK
#
# http://kbdlayout.info/KBDTUQ/overview+names?arrangement=OADG109A

# C64 keyboard matrix:
#
#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+

# C64 Keyboard layout:
#
#   arrow 1!  2"  3#  4$  5%  6&  7'  8(  9)  0   +   -   pound clr del     f1/f2
#    ctrl   q   w   e   r   t   y   u   i   o   p   @   *   ^   restore     f3/f4
#   r/s SL    a   s   d   f   g   h   j   k   l   :[  ;]  =   return        f5/f6
#   CBM LS      z   x   c   v   b   n   m   ,<  .>  /?  RS  u/d l/r         f7/f8
#                               space

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT
!LCBM 7 5
!VCBM LCBM
!LCTRL 7 2
!VCTRL LCTRL

#####################
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|

BackSpace       0 0 8
Return          0 1 8
Left            0 2 1
Right           0 2 8
F7              0 3 8
F8              0 3 1
F1              0 4 8
F2              0 4 1
F3              0 5 8
F4              0 5 1
F5              0 6 8
F6              0 6 1
Down            0 7 8
Up              0 7 1

#####################
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |

dead_circumflex 1 0 8
plus            1 3 8
Shift_L         1 7 2
# shift lock
Caps_Lock       1 7 64

#####################
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |

percent         2 0 8
ampersand       2 3 8

#####################
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |

slash           3 0 8
parenleft       3 3 8

#####################
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |

parenright      4 0 8
equal           4 3 8

#####################
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |

asterisk        5 0 8
question        5 0 8
minus           5 3 8
underscore      5 3 8
ccedilla        5 4 8
Ccedilla        5 4 1
scedilla        5 5 8
Scedilla        5 5 8
gbreve          5 6 8
Gbreve          5 6 8
odiaeresis      5 7 8
Odiaeresis      5 7 8

#####################
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |

Insert          6 0 8
udiaeresis      6 1 8
Udiaeresis      6 1 8
i               6 2 8
Iabovedot       6 2 8
Home            6 3 8
Shift_R         6 4 4
comma           6 5 8
semicolon		6 5 8
Delete          6 6 8
period          6 7 8
colon           6 7 8

#####################
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |

exclam          7 0 8
# grave / tilde -> arrow left
quotedbl        7 1 8
eacute          7 1 8
# Tab = CTRL
Tab             7 2 16392
# Shift + Tab = CTRL
ISO_Left_Tab    7 2 16392
apostrophe      7 3 8
space           7 4 8
# Control_L = CBM
Control_L       7 5 8200
Escape          7 7 8

#####################
# letters and numbers

0 4 3 8
1 7 0 8
2 7 3 8
3 1 0 8
4 1 3 8
5 2 0 8
6 2 3 8
7 3 0 8
8 3 3 8
9 4 0 8

A 1 2 8
B 3 4 8
C 2 4 8
D 2 2 8
E 1 6 8
F 2 5 8
G 3 2 8
H 3 5 8
idotless 4 1 8
J 4 2 8
K 4 5 8
L 5 2 8
M 4 4 8
N 4 7 8
O 4 6 8
P 5 1 8
Q 7 6 8
R 2 1 8
S 1 5 8
T 2 6 8
U 3 6 8
V 3 7 8
W 1 1 8
X 2 7 8
Y 3 1 8
Z 1 4 8
a 1 2 8
b 3 4 8
c 2 4 8
d 2 2 8
e 1 6 8
f 2 5 8
g 3 2 8
h 3 5 8
I 4 1 8
j 4 2 8
k 4 5 8
l 5 2 8
m 4 4 8
n 4 7 8
o 4 6 8
p 5 1 8
q 7 6 8
r 2 1 8
s 1 5 8
t 2 6 8
u 3 6 8
v 3 7 8
w 1 1 8
x 2 7 8
y 3 1 8
z 1 4 8

# Restore key mappings
Page_Up -3 0
F12 -3 0
Prior -3 1

#
# joyport attached keypad
#
Num_Lock    -5 0
KP_7        -5 1
KP_8        -5 2
KP_9        -5 3
KP_Divide   -5 4
Scroll_Lock -5 5
KP_4        -5 6
KP_5        -5 7
KP_6        -5 8
KP_Multiply -5 9
Sys_Req     -5 10
KP_1        -5 11
KP_2        -5 12
KP_3        -5 13
KP_Subtract -5 14
Print       -5 15
KP_0        -5 16
KP_Delete   -5 17
KP_Enter    -5 18
KP_Add      -5 19
