# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal lines have 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
#  for emulated keyboards that have only one shift key, set both LSHIFT
#  and RSHIFT to the same row/col and use RSHIFT for VSHIFT and SHIFTL.
# '!LCTRL row col'       left control keyboard row/column
# '!VCTRL ctrlkey'       virtual control key (LCTRL)
# '!LCBM row col'        left CBM keyboard row/column
# '!VCBM cbmkey'         virtual CBM key (LCBM)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have these values, flags can be ORed to combine them:
# 0x0000      0  key is not shifted for this keysym/scancode
# 0x0001      1  key is combined with shift for this keysym/scancode
# 0x0002      2  key is left shift on emulated machine
# 0x0004      4  key is right shift on emulated machine (use only this one
#                for emulated keyboards that have only one shift key)
# 0x0008      8  key can be shifted or not with this keysym/scancode
# 0x0010     16  deshift key for this keysym/scancode
# 0x0020     32  another definition for this keysym/scancode follows
# 0x0040     64  key is shift-lock on emulated machine
# 0x0080    128  shift modifier required on host
# 0x0100    256  key is used for an alternative keyboard mapping, e.g. C64 mode in x128
# 0x0200    512  alt-r (alt-gr) modifier required on host
# 0x0400   1024  ctrl modifier required on host
# 0x0800   2048  key is combined with cbm for this keysym/scancode
# 0x1000   4096  key is combined with ctrl for this keysym/scancode
# 0x2000   8192  key is (left) cbm on emulated machine
# 0x4000  16384  key is (left) ctrl on emulated machine
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key (x128)
# 'keysym -4 1' CAPS (ASCII/DIN) key (x128)
# 'keysym -5 n' joyport keypad, key n (not supported in x128)
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Positional Mapping for Individual Computer's "Keyrah", US Layout, C64, GTK

# to use this keymap with keyrah
# - host keyboard mapping should be "us"
# - the jumper in keyrah should be set to "us"
# - switch in position "down" (emulator)
# - set joystick port 1 to "keyset a" and port 2 to "keyset b"

# C64 keyboard matrix:
#
#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+

# C64 Keyboard layout:
#
#   arrow 1!  2"  3#  4$  5%  6&  7'  8(  9)  0   +   -   pound clr del     f1/f2
#    ctrl   q   w   e   r   t   y   u   i   o   p   @   *   ^   restore     f3/f4
#   r/s SL    a   s   d   f   g   h   j   k   l   :[  ;]  =   return        f5/f6
#   CBM LS      z   x   c   v   b   n   m   ,<  .>  /?  RS  u/d l/r         f7/f8
#                               space

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT
!LCBM 7 5
!VCBM LCBM
!LCTRL 7 2
!VCTRL LCTRL

#####################
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|

# inst/del
BackSpace        0 0 8
# return
Return           0 1 8
# cursor r/l
Right            0 2 8
Left             0 2 1
# f7
F7               0 3 8
F8               0 3 1
# f1
F1               0 4 8
F2               0 4 1
# f3
F3               0 5 8
F4               0 5 1
# f4
F5               0 6 8
F6               0 6 1
# cursor u/d
Up               0 7 1
Down             0 7 8

#####################
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |

# shift+3
numbersign       1 0 8
# shift+4
dollar           1 3 8
# left shift
Shift_L          1 7 2
# shift lock
Caps_Lock        1 7 64

#####################
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |

# shift+5
percent          2 0 8
# shift+6
asciicircum      2 3 8
dead_circumflex  2 3 8

#####################
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |

# shift+7
ampersand        3 0 8
# shift+8
asterisk         3 3 8

#####################
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |

# shift+9
parenleft        4 0 8
# shift+0
equal            4 3 8

#####################
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |

# plus
minus            5 0 8
underscore       5 0 1
# minus
equal            5 3 8
plus             5 3 1
# dot
period           5 4 8
greater          5 4 1
# colon
semicolon        5 5 8
colon            5 5 1
# @-key
bracketleft      5 6 8
braceleft        5 6 1
# comma
comma            5 7 8
less             5 7 1

#####################
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |

# pound
Insert           6 0 8
# *
bracketright     6 1 8
braceright       6 1 1
# semi-colon
apostrophe       6 2 8
quotedbl         6 2 1
dead_diaeresis   6 2 8
dead_acute       6 2 16
# clr/home
Home             6 3 8
# right shift
Shift_R          6 4 4
# =
backslash        6 5 8
bar              6 5 1
# arrow up / pi
Delete           6 6 8
# / ?
slash            6 7 8
question         6 7 1

#####################
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |

# shift+1
exclam           7 0 8
# left arrow
grave            7 1 8 
asciitilde       7 1 1
dead_grave       7 1 8 
dead_perispomeni 7 1 1
# ctrl
Tab              7 2 16392
ISO_Left_Tab     7 2 16392
# shift+2
at               7 3 8
# space
space            7 4 8
# cbm
Control_L        7 5 8200
# run/stop
Escape           7 7 8

#####################
# letters and numbers

0 4 3 8
1 7 0 8
2 7 3 8
3 1 0 8
4 1 3 8
5 2 0 8
6 2 3 8
7 3 0 8
8 3 3 8
9 4 0 8

A 1 2 8
B 3 4 8
C 2 4 8
D 2 2 8
E 1 6 8
F 2 5 8
G 3 2 8
H 3 5 8
I 4 1 8
J 4 2 8
K 4 5 8
L 5 2 8
M 4 4 8
N 4 7 8
O 4 6 8
P 5 1 8
Q 7 6 8
R 2 1 8
S 1 5 8
T 2 6 8
U 3 6 8
V 3 7 8
W 1 1 8
X 2 7 8
Y 3 1 8
Z 1 4 8
a 1 2 8
b 3 4 8
c 2 4 8
d 2 2 8
e 1 6 8
f 2 5 8
g 3 2 8
h 3 5 8
i 4 1 8
j 4 2 8
k 4 5 8
l 5 2 8
m 4 4 8
n 4 7 8
o 4 6 8
p 5 1 8
q 7 6 8
r 2 1 8
s 1 5 8
t 2 6 8
u 3 6 8
v 3 7 8
w 1 1 8
x 2 7 8
y 3 1 8
z 1 4 8

#
# Restore key
#
Prior -3 0

#
# joystick port 1
#
KP_0    -1 0
KP_9    -1 7
KP_3    -1 2
KP_7    -1 4
KP_1    -1 5

#
# joystick port 2
#
KP_5    -2 0
KP_8    -2 7
KP_2    -2 2
KP_4    -2 4
KP_6    -2 5 

#
# joyport attached keypad
#
Num_Lock    -5 0
KP_7        -5 1
KP_8        -5 2
KP_9        -5 3
KP_Divide   -5 4
Scroll_Lock -5 5
KP_4        -5 6
KP_5        -5 7
KP_6        -5 8
KP_Multiply -5 9
Sys_Req     -5 10
KP_1        -5 11
KP_2        -5 12
KP_3        -5 13
KP_Subtract -5 14
Print       -5 15
KP_0        -5 16
KP_Delete   -5 17
KP_Enter    -5 18
KP_Add      -5 19
