# VICE keyboard mapping file
#
# A Keyboard map is read in as patch to the current map.
#
# File format:
# - comment lines start with '#'
# - keyword lines start with '!keyword'
# - normal lines have 'keysym/scancode row column shiftflag'
#
# Keywords and their lines are:
# '!CLEAR'               clear whole table
# '!INCLUDE filename'    read file as mapping file
# '!LSHIFT row col'      left shift keyboard row/column
# '!RSHIFT row col'      right shift keyboard row/column
# '!VSHIFT shiftkey'     virtual shift key (RSHIFT or LSHIFT)
# '!SHIFTL shiftkey'     shift lock key (RSHIFT or LSHIFT)
#  for emulated keyboards that have only one shift key, set both LSHIFT
#  and RSHIFT to the same row/col and use RSHIFT for VSHIFT and SHIFTL.
# '!LCTRL row col'       left control keyboard row/column
# '!VCTRL ctrlkey'       virtual control key (LCTRL)
# '!LCBM row col'        left CBM keyboard row/column
# '!VCBM cbmkey'         virtual CBM key (LCBM)
# '!UNDEF keysym'        remove keysym from table
#
# Shiftflag can have these values, flags can be ORed to combine them:
# 0x0000      0  key is not shifted for this keysym/scancode
# 0x0001      1  key is combined with shift for this keysym/scancode
# 0x0002      2  key is left shift on emulated machine
# 0x0004      4  key is right shift on emulated machine (use only this one
#                for emulated keyboards that have only one shift key)
# 0x0008      8  key can be shifted or not with this keysym/scancode
# 0x0010     16  deshift key for this keysym/scancode
# 0x0020     32  another definition for this keysym/scancode follows
# 0x0040     64  key is shift-lock on emulated machine
# 0x0080    128  shift modifier required on host
# 0x0100    256  key is used for an alternative keyboard mapping, e.g. C64 mode in x128
# 0x0200    512  alt-r (alt-gr) modifier required on host
# 0x0400   1024  ctrl modifier required on host
# 0x0800   2048  key is combined with cbm for this keysym/scancode
# 0x1000   4096  key is combined with ctrl for this keysym/scancode
# 0x2000   8192  key is (left) cbm on emulated machine
# 0x4000  16384  key is (left) ctrl on emulated machine
#
# Negative row values:
# 'keysym -1 n' joystick keymap A, direction n
# 'keysym -2 n' joystick keymap B, direction n
# 'keysym -3 0' first RESTORE key
# 'keysym -3 1' second RESTORE key
# 'keysym -4 0' 40/80 column key (x128)
# 'keysym -4 1' CAPS (ASCII/DIN) key (x128)
# 'keysym -5 n' joyport keypad, key n (not supported in x128)
#
# Joystick direction values:
# 0      Fire
# 1      South/West
# 2      South
# 3      South/East
# 4      West
# 5      East
# 6      North/West
# 7      North
# 8      North/East
#
# Joyport keypad key layout:
# --------------------------
# |  0 |  1 |  2 |  3 |  4 |
# --------------------------
# |  5 |  6 |  7 |  8 |  9 |
# --------------------------
# | 10 | 11 | 12 | 13 | 14 |
# --------------------------
# | 15 | 16 | 17 | 18 | 19 |
# --------------------------
#
# When a bigger spaced key is used,
# it uses the upper left most key value.

# Positional Mapping, V128 Custom Keyboard Layout, C128, SDL

# note: For some reason SDL does not get keyboard events for "dead keys" at all,
#       so a "nodeadkeys" layout must be used. CAUTION: apparently SDL generates
#       some tables internally at startup - switching the host layout while
#       the emulator is running produces unpredictable results (broken keycodes)

# C128 Keyboard matrix
#
#       +-----+-----+-----+-----+-----+-----+-----+-----+
#       |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 0| DEL |Retrn|C_L/R|  F7 |  F1 |  F3 |  F5 |C_U/D|
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 1| 3 # |  W  |  A  | 4 $ |  Z  |  S  |  E  | S_L |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 2| 5 % |  R  |  D  | 6 & |  C  |  F  |  T  |  X  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 3| 7 ' |  Y  |  G  | 8 ( |  B  |  H  |  U  |  V  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 4| 9 ) |  I  |  J  |  0  |  M  |  K  |  O  |  N  |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 5|  +  |  P  |  L  |  -  | . > | : [ |  @  | , < |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 6|POUND|  *  | ; ] | HOME| S_R |  =  | A_UP| / ? |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 7| 1 ! |A_LFT| CTRL| 2 " |SPACE|  C= |  Q  | R/S |
# +-----+-----+-----+-----+-----+-----+-----+-----+-----+
#
#        +-----+-----+-----+-----+-----+-----+-----+-----+
#        |Bit 0|Bit 1|Bit 2|Bit 3|Bit 4|Bit 5|Bit 6|Bit 7|
# +------+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 8 |HELP | KP 8| KP 5| TAB | KP 2| KP 4| KP 7| KP 1|
# +------+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 9 | ESC | KP +| KP -| LF  |KP CR| KP 6| KP 9| KP 3|
# +------+-----+-----+-----+-----+-----+-----+-----+-----+
# |Bit 10| ALT | KP 0| KP .|A.UP |A.DWN|A.LFT|A.RGT|NOSCR|
# +------+-----+-----+-----+-----+-----+-----+-----+-----+

# C128 Keyboard layout:
#
#   ESC TAB ALT CAPS       HELP L/F 40/80 NOSCRL     up down left right  F1/2 F3/4 F5/6 F7/8
#
#   arrow 1!  2"  3#  4$  5%  6&  7'  8(  9)  0   +   -   pound clr del     7   8   9   +
#    ctrl   q   w   e   r   t   y   u   i   o   p   @   *   ^   restore     4   5   6   -
#   r/s SL    a   s   d   f   g   h   j   k   l   :[  ;]  =   return        1   2   3   enter
#   CBM LSHFT   z   x   c   v   b   n   m   ,<  .>  /?  RSHFT   u/d l/r     0       .
#                               SPACE

!CLEAR
!LSHIFT 1 7
!RSHIFT 6 4
!VSHIFT RSHIFT
!SHIFTL LSHIFT
!LCBM 7 5
!VCBM LCBM
!LCTRL 7 2
!VCTRL LCTRL

# Main keyboard keys
96 7 1 8                /*            ` -> Left Arrow   */
49 7 0 8                /*            1 -> 1            */
50 7 3 8                /*            2 -> 2            */
51 1 0 8                /*            3 -> 3            */
52 1 3 8                /*            4 -> 4            */
53 2 0 8                /*            5 -> 5            */
54 2 3 8                /*            6 -> 6            */
55 3 0 8                /*            7 -> 7            */
56 3 3 8                /*            8 -> 8            */
57 4 0 8                /*            9 -> 9            */
48 4 3 8                /*            0 -> 0            */
45 5 0 8                /*        Minus -> Plus         */
61 5 3 8                /*        Equal -> Minus        */
8 0 0 8                 /*    Backspace -> Del          */
9 7 2 16384             /*          TAB -> Ctrl         */
113 7 6 8               /*            Q -> Q            */
119 1 1 8               /*            W -> W            */
101 1 6 8               /*            E -> E            */
114 2 1 8               /*            R -> R            */
116 2 6 8               /*            T -> T            */
121 3 1 8               /*            Y -> Y            */
117 3 6 8               /*            U -> U            */
105 4 1 8               /*            I -> I            */
111 4 6 8               /*            O -> O            */
112 5 1 8               /*            P -> P            */
91 5 6 8                /*            [ -> @            */
93 6 1 8                /*            ] -> *            */
13 0 1 8                /*       Return -> Return       */
306 7 5 8192            /*    Left Ctrl -> CBM          */
301 1 7 64              /*    Caps Lock -> SHIFT LOCK   */
97 1 2 8                /*            A -> A            */
115 1 5 8               /*            S -> S            */
100 2 2 8               /*            D -> D            */
102 2 5 8               /*            F -> F            */
103 3 2 8               /*            G -> G            */
104 3 5 8               /*            H -> H            */
106 4 2 8               /*            J -> J            */
107 4 5 8               /*            K -> K            */
108 5 2 8               /*            L -> L            */
59 5 5 8                /*            ; -> :            */
39 6 2 8                /*            ' -> ;            */
92 6 5 8                /*            \ -> =            */
304 1 7 2               /*   Left Shift -> Left Shift   */
122 1 4 8               /*            Z -> Z            */
120 2 7 8               /*            X -> X            */
99 2 4 8                /*            C -> C            */
118 3 7 8               /*            V -> V            */
98 3 4 8                /*            B -> B            */
110 4 7 8               /*            N -> N            */
109 4 4 8               /*            M -> M            */
44 5 7 8                /*            , -> ,            */
46 5 4 8                /*            . -> .            */
47 6 7 8                /*            / -> /            */
303 6 4 4               /*  Right Shift -> Right Shift  */
32 7 4 8                /*        Space -> Space        */

# Function keys
27 7 7 8                /*          ESC -> Run/Stop     */
282 9 0 8               /*           F1 -> ESC          */
283 8 3 8               /*           F2 -> TAB          */
284 0 10 0              /*           F3 -> ALT          */
285 -5 1                /*           F4 -> CAPS         */
286 8 0 8               /*           F5 -> HELP         */
287 9 3 8               /*           F6 -> LINE FEED    */
288 -4 0                /*           F7 -> 40/80        */
289 10 7 8              /*           F8 -> NO SCROLL    */
290 0 4 8               /*           F9 -> F1/F2        */
291 0 5 8               /*          F10 -> F3/F4        */
292 0 6 8               /*          F11 -> F5/F6        */
293 0 3 8               /*          F12 -> F7/F8        */

# Cursor keys
274 0 7 8               /*  Cursor Down -> Cursor Down  */
276 0 2 1               /*  Cursor Left -> Cursor Left  */
275 0 2 8               /* Cursor Right -> Cursor Right */
273 0 7 1               /*    Cursor Up -> Cursor Up    */

# Navigation cluster
277 6 0 8               /*          Ins -> Pound        */
278 6 3 8               /*         Home -> CLR/HOME     */
280 -3 0                /*         PgUp -> RESTORE      */
127 6 6 8               /*          Del -> Up Arrow     */

# Keypad
263 8 6 8               /*     Numpad 7 -> Numpad 7     */
264 8 1 8               /*     Numpad 8 -> Numpad 8     */
265 9 6 8               /*     Numpad 9 -> Numpad 9     */
269 9 1 8               /*     Numpad - -> Numpad +     */
260 8 5 8               /*     Numpad 4 -> Numpad 4     */
261 8 2 8               /*     Numpad 5 -> Numpad 5     */
262 9 5 8               /*     Numpad 6 -> Numpad 6     */
270 9 2 8               /*     Numpad + -> Numpad -     */
257 8 7 8               /*     Numpad 1 -> Numpad 1     */
258 8 4 8               /*     Numpad 2 -> Numpad 2     */
259 9 7 8               /*     Numpad 3 -> Numpad 3     */
256 10 1 8              /*     Numpad 0 -> Numpad 0     */
266 10 2 8              /*     Numpad . -> Numpad .     */
271 9 4 8               /* Numpad Enter -> Numpad Enter */

